{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":13,"rows_kept":13,"merged":[[0,0,0,12],[1,0,1,12],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,2,11],[2,12,4,12],[3,6,3,8],[3,9,4,9],[3,10,4,10],[3,11,4,11],[11,1,11,11],[12,0,12,12]]}
["维修工程项目报价表"]
["项目名称：业务大厅改造电路                                                       报价单位："]
["序号","项目名称","项目描述特征","计量单位","工程量","综合单价","综合单价包括内容",{"$nulls":5},"合  价(元）"]
[{"$nulls":6},"材料",null,null,"人工费","机械费","安全措施费"]
[{"$nulls":6},"品种(品牌）","规格、型号","单价"]
[1,"原有照明灯调整高度","将原有20套照明灯安装高度降低50cn—100cm","套",20,null,"金卤灯"]
[2,"改造、新增供电线路","改造及新增电源线、控制线、控制开关箱及电线套管","项",1]
[3,"室内高空作业车租赁","满足10m-12m作业高度的室内作业车租赁费","项",1]
[4,"成品保护","施工作业过程中对原有地面保护，使用不少于2层竹木模板，确保承重不小于4吨","项",1]
[5]
[6]
[7,"本页合计",{"$nulls":10},{"$f":"SUM(M6:M11)","v":0}]
["备注：该报价应该综合考虑安全措施费、意外保险费、设备进出场费、税金等。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}